***JL Precision***

## Shear, Punch, Laser and Forming Equipment:

Laser Cutters (x3) Turret Punches (x3) Press Brakes (x9) Rollers (x2)

Shears / Saws

## Milling and Turning Equipment:

4-Axis CNC Horizontals (x2) Verticals CNC (x9)

CNC Lathes (x2) Manual Equipment

**AMADA FOM2 3015 NT**

**4KW laser cuts 0.875” CRS**

**0.5” SS, 0.375” Al**

**AMADA EMK 3610NT**

**600 ton press brake, bends up to 23’**

## Welding

MIG

TIG

Structural Framing

## Quick Turn Finishing and Plating

Anodize: Type II and III

Alodine: Clear, Gold, and Chrome-Free Nickel: Bright and Electroless Passivation

Zinc: Clear and Gold

**HAAS VF11**

**120” x 42” x 35” table**



## Painting and Surface Preparation

Bead Blast Powder Coating Wet Painting Silk Screening